Daytona Cobra Coupe

**Driven by John & Helen Saia**

|  |  |
| --- | --- |
| * Factory Five Daytona Cobra Coupe tribute * Built period-correct – all-new components * 392 Ford Motorsports engine – 425 HP/450 lb.-ft. torque * Ford Racing GT40 aluminum cylinder heads * Forged pistons and forged steel connecting rods * Hydraulic roller camshaft and rockers: .583/.563 lift * 48 IDA Weber carburetors * MSD ignition and billet MSD distributor | * Guardsman Blue with Wimbledon White stripes * Four wheel fully independent coil-over suspension * Knockoff wheels – 7.5” X 15” – front; 9.5” X 15” – rear * Tires – P235/60 R15 – front; P295/50 R15 – rear * Tremec T-56 five-speed transmission * Independent T-Bird carrier & 3.41 differential * Stewart Warner gauges * Removable Cobra steering wheel |

